(export (version D)
  (design
    (source /home/arofarn/Make/Cameteo/Serial-SHIM/Serial-SHIM.sch)
    (date "jeu. 21 sept. 2017 19:02:46 CEST")
    (tool "Eeschema 4.0.2+dfsg1-stable")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Serial-SHIM.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref Serial1)
      (value CONN_01X04)
      (footprint Socket_Strips:Socket_Strip_Angled_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 59BCE9F7))
    (comp (ref PI-GPIO1)
      (value CONN_02X05)
      (footprint Pin_Headers:Pin_Header_Straight_2x05)
      (libsource (lib conn) (part CONN_02X05))
      (sheetpath (names /) (tstamps /))
      (tstamp 59BCEAE4)))
  (libparts
    (libpart (lib conn) (part CONN_01X04)
      (description "Connector 01x04")
      (footprints
        (fp Pin_Header_Straight_1X04)
        (fp Pin_Header_Angled_1X04)
        (fp Socket_Strip_Straight_1X04)
        (fp Socket_Strip_Angled_1X04))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib conn) (part CONN_02X05)
      (description "Connector 02x05")
      (footprints
        (fp Pin_Header_Straight_2X05)
        (fp Pin_Header_Angled_2X05)
        (fp Socket_Strip_Straight_2X05)
        (fp Socket_Strip_Angled_2X05))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_02X05))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive)))))
  (libraries
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib)))
  (nets
    (net (code 1) (name "Net-(PI-GPIO1-Pad10)")
      (node (ref Serial1) (pin 4))
      (node (ref PI-GPIO1) (pin 10)))
    (net (code 3) (name +5V)
      (node (ref PI-GPIO1) (pin 4))
      (node (ref Serial1) (pin 1))
      (node (ref PI-GPIO1) (pin 2)))
    (net (code 4) (name "Net-(PI-GPIO1-Pad1)")
      (node (ref PI-GPIO1) (pin 1)))
    (net (code 5) (name "Net-(PI-GPIO1-Pad3)")
      (node (ref PI-GPIO1) (pin 3)))
    (net (code 6) (name "Net-(PI-GPIO1-Pad5)")
      (node (ref PI-GPIO1) (pin 5)))
    (net (code 7) (name "Net-(PI-GPIO1-Pad7)")
      (node (ref PI-GPIO1) (pin 7)))
    (net (code 8) (name "Net-(PI-GPIO1-Pad9)")
      (node (ref PI-GPIO1) (pin 9)))
    (net (code 9) (name "Net-(PI-GPIO1-Pad6)")
      (node (ref Serial1) (pin 2))
      (node (ref PI-GPIO1) (pin 6)))
    (net (code 10) (name "Net-(PI-GPIO1-Pad8)")
      (node (ref Serial1) (pin 3))
      (node (ref PI-GPIO1) (pin 8)))))